# Process:

First of all I needed to remember everything related to timers,

So I first watched timer videos of this play list:

<https://www.youtube.com/watch?v=Sr7aYoWgMbg&list=PLoiqjtgvXf9e2VJk8GWEXwECPM_7JRwkE&index=32>

# Content:

Here I will be writing all the content I need to cover in the timer session:

First of all we need to revise what’s a clk in a microprocessor:

Clk is the ticks that are digital square waves which make microprocess progress through its functionality like executing line-by-line code that helps the microprocessor to keep in track

In short it’s like a heart beat for us humans.

The clk has a period which we call a microprocessor clk or a tick which is usually very quick like some micro seconds or even faster.

Ok now let’s talk about timers:

First of all it’s a prephiral so we will find itsdriver in the MCALlayer

Like any other prephiral it has:

* HW circuit : that contains of system clk and prescaler

A prescaler it’s just a frequency divider that means it slows down the system clock

So

* Register: where we can control this prephiral and we will be using systick register

The timer hardware circuit has two modes:

1. Timer mode: which is just a timer like a stop watch if the time run out it will do an interrupt so this is periodic and internal
2. Counter mode: Which just used as a counter here you could use like an external switch to count from the user so this is not periodic and external

Now as for the register:

It contains R= 8 or 10 bit for counting as it stores the # of ticks, and has an enable pin attached to an or gate which is used to determine which mode you will use

So we can say that the total time: